The Effect of Pressurization Rate and Pattern on Injection-induced Seismicity in Porous Media: An Experimental Study
=============
Data and Figures
------
All data related to triaxial injection-driven fault reactivation, including measured displacement, stress, load, etc., are stored in Excel files. 
These files contain both raw data from mechanical loading parameters and processed data used to create the figures in this paper or chapter. 
In addition to mechanical data, passive acoustic data, such as the maximum amplitude of each event and the cumulative number of acoustic emission (AE) events, are also recorded in each Excel file. 
Note that five distinct datasets are provided through five Excel files, each corresponding to one of the experiments conducted in this study.

All figures can be plotted using the processed data included in the Excel files for each experiment.

Author
------

* Milad Naderloo
  *Delft University of Technology, Section of Civil Engineering and Ceosciences, Delft, Netherlands*
