*** Clarity on Fruitfrost ***
Authors: J.Boekee [1], D. Yi [2], M ten Veldhuis [1], B. van de Wiel [2]
[1] Faculty of Civil Engineering and Geosciences, Department of Water Resources, 
[2] Faculty of Civil Engineering and Geosciences, Department of Geoscience and Remote Sensing
Delft University of Technology
Corresponding author: B. van de Wiel
Contact Information: 
b.j.h.vandewiel@tudelft.nl
Delft University of Technology - Faculty of Civil Engineering and Geosciences
P.O. Box 5058
2600 GA Delft
The Netherlands

***General Introduction***
This dataset contains data collected during the Clarity on Fruitfrost project at Delft University of Technology, as part of J. Boekee's PhD Thesis project.
It is being made public both to act as supplementary data for publications of J. Boekee and in order for other researchers to use this data in their own work.
The data in this data set was collected in Wageningen, The Netherlands, on 04-05-2022 till 24-05-2022.
This research project was made possible by a grant from the NWO.

***Purpose of the measurement campaign***
The purpose of these experiments was to study the temperature profiles in the roughness sublayer over grass of different heights.

***Description of the data in this data set***
The data included in this dataset includes DTS measurements in a harp (DTS_harp.nc) and mast (DTS_mast.nc) configuration, and measurements of the grass height (grassheight.csv).
Supporting data from the same measurement site and time period can be found at: https://veenkampen.nl/data/

Distributed Temperature Sensing: 	Ultima M, 1.6mm cable
					2022-05-04T00:00 - 2022-05-24T23:00 (10 minute resolution)
					harp  0.02 - 0.64 m height
					tower 0.31 m - 8.699 m height 
					Units: Celcius
					Data: air temperature 

Grass height sections of the harp:	Undisturbed: 0.1 - 1.70 m
					20 cm: 1.70 – 3.55 m
					10 cm: 3.55 – 5.61 m
					3 cm:  5.61 – 7.70 m
