In the article related to this dataset, we report on the screen printing of stretchable, graphene-based conductors for use in wearable technology. The conductors remained conductive even under 100% strain and demonstrated high fatigue resistance to cyclic strains of 20-50%. Using photonic annealing, the sheet resistance of the printed conductors was reduced from ca 34 Ω □−1 mil−1 to <10 Ω □−1 mil−1, while the stretchability and fatigue resistance were preserved. This dataset contains the data and analysis scripts needed to reproduce the findings in the study.

In this repository, we have uploaded a zip folder for each figure and table, and a seperate folder for the data in the supplementary information. These folders contain the relevant raw and/or processed data and the code necessary to reproduce the figures and tables. The scripts contain the settings as used to calculate the results and obtain the figures from the paper, unless noted otherwise. In case of the scripts use to analyze the data from the strain tests, one Python file has been uploaded per sample included in the manuscript. These scripts therefore contain the correct parameters for each sample. The scripts have been annotated with explanations as much as possible.