Files in this dataset:

1 - Scenario Files:

	a - For manned aviation:
	
		manned_aviation_scenarios.7z
	
	b - For unmanned aviation:
	
		unmanned_aviation_scenarios.7z
		
	- Each .scn files refers to a scenario. Instxxx indicates the traffic density. Different trajectories are used for each traffic density; as
	  per Repx.
	  
	- File Batch-Heading-Normal-UA.scn can be called in order to run all scenario files in a batch.

	- areaDefinition.scn is used to format the area of the simulation. Aircraft are removed once they leave this area.
	
	- a settingsOFF.scn file should be added with indications of the properties of the simulation (ASAS ON, which CR to use, ...)

2 - Results Files:

	a - For manned aviation:
	
		manned_aviation_results.7z
		
	
	b - For unmanned aviation:
	
		unmanned_aviation_results.7z
		
	Files ASASDATA have the following data:
	
	Time Stamp [s], Number of aircraft [-], Number of current conflicts [-], Number of current LoS [-], Total number of conflicts [-], Total number of LoS [-] Intrusion per LoS pair [nm]
		
	Files FLSTLOG have the following data:
	
	Deletion Time [s], Call sign [-], Spawn Time [s], Flight time [s], Time in conflict [s], Actual Distance 2D [m], Work Done [J], Latitude,Longitude,Altitude [m], TAS [m/s],
	
	where:
	
	s - seconds
	nm - nautical miles
	m - meters
	J - joules
	
	All columns are separated by a comma (,).