***Ammonium recovery from digested blackwater using an electrochemical system combined with Donnan Dialysis***
Authors: Mariana Rodrigues a,b, Aishwarya Paradkar a, Tom Sleutels a, Annemiek ter Heijne b, Cees J.N. Buisman a,b, Hubertus V.M. Hamelers a,b, Philipp Kuntke a,b*
a Wetsus, European Centre of Excellence for Sustainable Water Technology, Oostergoweg 9, 8911MA Leeuwarden; P.O. Box 1113, 8900 CC Leeuwarden, The Netherlands
b Environmental Technology, Wageningen University, Bornse Weilanden 9, 6708 WG Wageningen;  P.O. Box 17, 6700 AA Wageningen, The Netherlands
Corresponding author: philipp.kuntke@wur.nl 
***General Introduction***
This dataset contains data collected during experiments on nitrogen recovery using electrodialysis combined with donnan dialysys. It is being made public both to act as supplementary data for publication and in order for other researchers to use this data in their own work.
This work was performed in Wetsus, European Centre of Excellence for Sustainable Water Technology, between September 2019 and March 2020. This work was also supported by the LIFE-NEWBIES project (LIFE17 ENV/NL/000408).
File: LIMS_analytical results.csv - includes the analytes measured from the influent, effluent Donnan dialysis, effluent (ED effluent), concentrate, cathode and acid solution of all different experiments as indicated in the "description" column
File: LN 0.5 blackwater with DD.csv - includes the data recorded every minute by the data logger when the combined system (electrodialysis+Donnan dialysis) was operated at Load Ratio 0.5 with digested blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1 blackwater with DD.csv - includes the data recorded every minute by the data logger when the combined system (electrodialysis+Donnan dialysis) was operated at Load Ratio 1 with digested blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1.3 blackwater with DD.csv - includes the data recorded every minute by the data logger when the combined system (electrodialysis+Donnan dialysis) was operated at Load Ratio 1.3 with digested blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1.5 blackwater with DD.csv - includes the data recorded every minute by the data logger when the combined system (electrodialysis+Donnan) dialysis was operated at Load Ratio 1.5 with digested blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1 blackwater without DD.csv - includes the data recorded every minute by the data logger when the single system (electrodialysis) was operated at Load Ratio 0.5 with digested blackwater). The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1 synthetic blackwater with DD.csv - includes the data recorded every minute by the data logger when the combined system (electrodialysis+Donnan dialysis) was operated at Load Ratio 1 with synthetic blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.
File: LN 1 synthetic blackwater without DD.csv - includes the data recorded every minute by the data logger when the single system (electrodialysis) was operated at Load Ratio 1 with synthetic blackwater. The recorded variables were: Data/time; Date time; E_HRES_Cathode; E_HRES_feed; HRES cat cond; HRES Feed cond; I EC2; I HRES; pH cat; pH Con; pH feed; t cat; t feed; Temp con; V EC2; V HRES.

All calculations are included in the manuscript. DOI: to be added
Data specific information:
E_HRES_Cathode (cathode measured potential); E_HRES_feed v A (anode measured potential); V EC2 (support cell voltage); HRES (cell voltage)  	unit Volts
HRES cat cond - cathode conductivity;HRES Feed cond (feed conductivity)				unit mS/cm
I EC2 (support cell current); I HRES (cell current)						unit Amperes 
pH cat (cathode pH);	pH Con (concentrate pH); pH feed (feed pH)	
t cat (cathode temperature); t feed (feed temperature); Temp con (concentrate temperature)					unit Celsius
Analyte i (i=species in solution)				unit mg/L
