*** EDoM measurement campaign: data from stationary boats ***
Authors: Bas van Maren, Julia Vroom, Daan van Keulen, Christian Maushake, Jan-Willem Mol, Theo Gerkema
Corresponding author: bas.vanmaren@deltares.nl

*** GENERAL INFORMATION ***
Subset of larger dataset collected during the Ems Dollard Measurements (EDoM) Campaign in 2018 and 2019. This subset contains data collected by stationary boats measuring for 13 hours on one location (one downward looking ADCP and a CTD with OBS casting every half hour)
It is composed of 6 files, each file containing the measurements collected on one location (3 in total) during one field campaign (2 in total). 

Filenemame convention: SB_<loc>_<year>.nc, where 
- SB is Stationary Boat, 
- <loc> is the location (EMD, EFW, GEI), 
- <year> is 2018 or 2019. 
See accompanying report(report-EDoM_v2.0.pdf) for location of stations.


*** METHODOLOGICAL INFORMATION ***
See accompanying report(report-EDoM_v2.0.pdf) for details.

*** DATA SPECIFIC INFORMATION ***

Each file contains
1. x
  description = "x-coordinate [m] (UTM 32)";  
  Units = "m";
2. y
  description = "y-coordinate [m] (UTM 32)";  
  Units = "m";
3. z_measures;
  description = "depth of bin center relative to device (shipboard adcp)";
  Units = "m";
4. time;
  description = "(Matlab) Serial date number  represents the whole and fractional number of days from 01-01-0000";  
  Units = "days since 01-01-0000";
5. Sal
  description = "salinity measurements interpolated on the adcp grid";
  Units = "ppt";
6. SSC
  description = "OBS measurements interpolated on the adcp grid";
  Units = "mg/l";
7. wlv;
  description = "water level elevation";
  Units = "m";
8. vel_East;
  description = "10 minute bin averaged velocity in the Eastward direction";
  Units = "m/s";
9. vel_North;
  description = "10 minute bin averaged velocity in the northward direction";
  Units = "m/s";  
