The file 'Supporting data for Experimental investigation of the in-plane cyclic behaviour of calcium silicate brick masonry walls.xlsx' contains two sheets.

Sheet 1. 'Complete VH-d curves' reports the recorded drifts of the walls (d) and the in-plane base shear force (VH) for eight walls tested in quasi-static cyclic conditions;
Sheet 2. 'Backbone VH-d curves' reports the backbone curve derived for each test. Each backbone curve is computed as the envelope of the cyclic curve provided in sheet 1.

Symbols:
d (%): drift of the wall, computed as the ratio between the wall net displacement (top displacement - base displacement) and the wall height 
VH (kN): in-plane shear, measured as reaction to the imposed net displacement